**Updating Headset Firmware Using Cable**

**Please DO NOT use the cable supplied with the headset for updating the firmware, as it is not designed to transfer data. Follow these steps:**

1. Install the *Config Tool* program using the installer provided in the archive. This installer includes the necessary files for updating the headset firmware.
   * **BE SURE** to first turn off the headset and disconnect the dongle from your PC.
2. Launch the *Config Tool* program.




1. Hold down the C button on the headset and insert the cable.





1. After launching the program, you will be asked to select the path to the file. Select the file that matches your model.



1. Click on the >> button and select *ADFU*.



1. Click on the drop-down list as in the screenshot and select *ADF*
2. To install, click the *Download* button.



1. Unplug the headset and enjoy!